**ORDER DESCRIPTION**

1. **Object of the contract**

The subject of the order is a supply of a mechanical elements as per specifications :

* Motorized XY Scanning Stage 1 pcs.

1. **Time-limit for completion of the contract**

**Completion deadline: as soon as possible, not later than 7 weeks from the date of placing the order.**

Deadline for completion of the order includes readiness to hand over the goods to the Ordering Party, which complies with application of the EXW Incoterms2020 principle.

According to the EXW (ex works) principle, the moment of delivery of the goods is considered to be the moment of placing the goods at the disposal of the buyer, at place indicated by the supplier (factory, plant etc.).

The Ordering Party shall accept application of other Incoterms2020 principle (such as FCA, DAP etc.), on condition that the Contractor will meet the deadline for completion, as referred to above.

1. **Parameters**

**5.1 Detailed scope of the subject**

| **Product name** | **Parameter** | **Specification** |
| --- | --- | --- |
| Motorized XY Scanning Stage | Travel range | 102x102 mm (4") |
| Lead screw pitch | 0.5 mm |
| Resolution | Full Step: 2.5 µm  1/8 step: 0.31 µm |
| Max speed | 10mm/sec |
| Load capacity | Horizontal: 50 kg  Vertical: 6 kg |

1. **Additional conditions related to the subject of the order.**
   1. Elements must be made in accordance with attached documentation.
   2. Elements must be made in given tolerances. If drawing contains not tolerated dimensions and there is no proper information on the drawing, elements shall be made in tolerance +/- 0.1mm.
   3. Elements must be made of materials indicated in drawing- tables.
   4. There is a quantity of elements needed to perform one set, indicated in each drawing-table, i.e. quantity of elements to perform means a number of pieces of one set multiplied by the number of sets.
   5. All of the elements delivered to the headquarters of the Contracting Party must be washed, ungreased. Elements must not contain any shavings or jagged edges, dents and other defects of the surface.
   6. All of the elements must be collated, packed in a way that secures elements from damaging in transport and storage.
   7. Elements will be randomly checked with certified measuring instruments in order to confirm compatibility of the elements with attached documentation. In case of incompatibility of the element with its documentation, the Contracting Party reserves the right to return the whole order to the Contractor to check and correct the elements.
   8. In case of failure to deliver a required quantity of elements or in case of delivery of elements made of the wrong materials, the Contracting Party will require the Contractor to perform the missing elements or to perform the elements of the right materials.
   9. Delivered goods must be factory new (I category – unused), meet the technologically-qualitative requirements determined by the manufacturer and be put on the market in accordance with the provisions of law in force on the territory of the Republic of Poland.