**W dniu 15.05.2020 r. Zamawiający zmienił treść zapytania ofertowego nr SDM-WS/14/2019 z dnia 9 maja 2020 r. w zakresie opisu przedmiotu zamówienia w następujący sposób.**

**Zamawiający przedłużył termin składania ofert do dnia 21 maja 2020 r.**

**Zapytanie ofertowe:**

1. **Punkt 3 – Szczegółowy zakres przedmiotu zamówienia.**

**Było:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| L.p. |  | Podzespół | Parametr/Funkcja | Opis |
| 1 | Parametry techniczne | Geometria maski | Grubość maski | * 120nm +/-10%
 |
| Wymiar maski | * 5” x 5” x 0,09”
 |
| Materiał | * Soda Lime lub Syntetyczna krzemionka topiona
 |
| Warstwa maskująca | Materiał | * Chrom
 |
| Grubość  | * 120nm +/-10%
 |
| Gęstość optyczna | * 3,0 +/- 0,3 @ 430nm
 |
| CD - Critical dimension- Wymiar krytyczny | Wymiar krytyczny | * 1µm
 |

**Jest:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| L.p. |  | Podzespół | Parametr/Funkcja | Opis |
|  |  | Geometria maski | Wymiar maski (S- szerokość x D- długość x W- wysokość) | * 5” x 5” x 0,09”
 |
| Materiał | * Soda Lime lub Syntetyczna krzemionka topiona
 |
| Warstwa maskująca | Materiał | * Chrom
 |
| Grubość  | * 120nm +/-10%
 |
| Gęstość optyczna | * 3,0 +/- 0,3 @ 430nm
 |
| CD - Critical dimension- Wymiar krytyczny | Wymiar krytyczny | * 1µm
 |

1. Punkt 8 - Termin składania ofert:

Było:

* 1. Termin składania ofert
1. Ofertę należy złożyć w terminie do dnia: 18 maja 2020 r.

Jest:

* 1. Termin składania ofert
1. **Ofertę należy złożyć w terminie do dnia: 21 maja 2020 r.**

**On 15.05.2020, the Employer changed the content of the request for quotation No. SDM-WS / 14/2019 of 9 May 2020 in the scope of the description of the subject of the order as follows.**

**The contracting authority extended the deadline for submission of offers to May 21, 2020.**

**Request of proposal:**

**1. Point 3 - Detailed scope of the contract.**

**Last:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| L.p. |  | subassembly | Parameter / Function | description |
| 1 | Technical specifications | Mask geometry | Mask thickness | * 120nm +/-10%
 |
| Mask size | * 5” x 5” x 0,09”
 |
| Material | * Soda Lime or Synthetic fused silica
 |
| Masking material | Material | * Chrom
 |
| Thickness | * 120nm +/-10%
 |
| Optical density | * 3,0 +/- 0,3 @ 430nm
 |
| CD - Critical dimension | Critical dimension | * 1µm
 |

**Now:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| L.p. |  | subassembly | Parameter / Function | description |
| 1 | Technical specifications | Mask geometry |  |  |
| Mask size (W- width x L- length x H- height) | * 5” x 5” x 0,09”
 |
| Material | * Soda Lime or Synthetic fused silica
 |
| Masking material | Material | * Chrom
 |
| Thickness | * 120nm +/-10%
 |
| Optical density | * 3,0 +/- 0,3 @ 430nm
 |
| CD - Critical dimension | Critical dimension | * 1µm
 |

**2. Point 8 - Deadline for submission of bids:**

It was:

8. Deadline for submission of bids

1. The offer should be submitted by: May 18, 2020.

Is:

8. Deadline for submission of bids

**1. The offer should be submitted by: May 21, 2020.**