**ORDER DESCRIPTION**

1. **Object of the contract**

The subject of the contract is a socket for TO66 header, in the amount of:

* Socket for a TO66 header 250 pcs.

1. **Parameters**

**5.1 Detailed scope of the subject**

| Product name | Parameter | Specification |
| --- | --- | --- |
| Socket for TO66 header | Dimensions | Pinholes circle diameter: 10.8 ± 0.05 mm |
| Number of pinholes: 9 |
| Pinholes position angle: 36° |
| Pinhole depth: 4 ± 1 mm |
| Acceptable pin diameter: 0.76 ± 0.1 mm |
| Mounting holes diameter: 3.8 ± 0.05 mm |
| Mounting holes spacing: 24.38 ± 0.2 mm |
| Mounting scheme compatibility | Through-hole technology |
| Insulator material | FR-4 epoxy |
| Terminal material | Brass |
| Contact material | BeCu |
|  | Terminal plating | Gold, 200 nm or thicker |
|  | Contact plating | Gold, 200 nm or thicker |